**EarthCam 61 MegapixelCam Robotic Model #ECAC06152 A&E Specifications**

**01.32.36 Video Monitoring and Documentation**

1. **CAMERA SPECIFICATIONS**
   1. **Contractor Contact Information**

The Contractor shall provide a Robotic High Definition Megapixel Webcam for users to remotely view the project on a secure connection via a network connection. The camera will provide a full view of the work area on the construction site.

CONTACT SYSTEM VENDOR: EarthCam Inc. / Brian Cury +1 201.488.1111

Email: WWW.EARTHCAM.NET/CONTACTUS

* 1. **Camera System for Highest Precision Monitoring and Documentation**
     + 1. Thermostatically controlled IP66/IP67 rated environmentally sealed black powder coated enclosure with stainless steel hardware
       2. User controlled window maintenance-free wiper to ensure clear images
       3. Industrial grade solid state embedded Linux System
       4. 61.0 Megapixels (9504 x 6336 pixels), Full Frame camera with a 35mm Exmor R CMOS Image Sensor
       5. Lens: F3.5-5.6 OSS, 28-70mm
       6. SONY optics for superior image quality
       7. Professional photo grade glass enclosure window
       8. Auto Features: ISO, Shutter, White Balance and Focus
       9. Live streaming video preview
       10. 567-point wide area autofocus system
       11. 425-point contrast detect points
       12. Rapid archiving capability with on demand image capture as fast as every 10 seconds for short term events
       13. Ultra-precise, Pan/Tilt robotic base designed to provide consistent imaging in all environments
       14. Pan/Tilt: Pan Range 360° Continuous Pan, Tilt: +45° to -90° pan mode
       15. Up to 1 Gigapixel (1000 megapixels) auto-generated 360° multilayer panoramas
       16. Communications: 10base-T/100base-TX Ethernet, IP Addressing: Dynamic or Static
       17. 4G cellular modem
       18. Smart diagnostic LED multi-color power indicator lamp
       19. 64GB On-Board Data Backup to provide a minimum of thirty days of on-board image retention
       20. Short term power device to send alerts if camera goes offline
       21. 120VAC, 220-230VAC
       22. Designed for EarthCam Control Center

1. **SERVICE SPECIFICATIONS**
   1. **Internet Based Online Interface**

The camera will be accessible via an internet based Software as a Service (SaaS) solution. This online interface will be managed and supported by the System Vendor. The service will be available for the term of the project and allow the viewing of live video and High Definition digital still images captured and stored of the project on both mobile and desktop platforms.

The Internet Based Online Interface shall include the following features:

* + 1. Responsive HTML5 design for cross-platform access on desktop and mobile devices
    2. Secure HTTPS compliant with live stream secured & encrypted via https transport
    3. Display project name and logo
    4. Project Dashboard allows easy navigation between multiple cameras and projects
    5. Real-time live video viewing with user-controllable Robotic Pan and Tilt
    6. User-controllable settings for creating and editing multiple preset compositions, each preset will be displayed as a thumbnail image
    7. Daily auto-generated 360° multilayer panoramas
    8. Onscreen control button for wiper and washer control to allow for remote cleaning of the viewing window
    9. Digital Pan, Tilt and Zoom capability within a High Definition images
    10. Custom tiling player to easily view High Definition panoramic images
    11. Instant live snapshot capability in addition to preset scheduled archives
    12. Visual timeline with quick thumbnail view allows image navigation by year, month, day and hour
    13. AI-edited time-lapse technology removes frames obscured by foreign objects or weather elements, with music and graphics then added for downloadable presentations
    14. Full Screen Mode for displaying complete image without any graphical frame
    15. Photo Filters and Graphical Markup Tools for detailing and creating notes with graphical overlays on images, including project title, logo and time date stamp
    16. Image Comparison Tool for comparing two images taken at different times, overlayed on top of each other
    17. Share Image Tool for saving, printing, emailing and posting to Hall of Fame
    18. Project Management Software integration (Autodesk Construction Cloud, Autodesk Build, CmiC, Esri, InEight, Infotech, Procore, Projectmates, Raken, Salesforce)
    19. 3D/4D Model Integration (Autodesk Navisworks, Autodesk Revit, Bentley Synchro)
    20. Social Media Integration Tools for sharing project images and notes
    21. Automatically generated daily/weekly project progress update email with camera image and weather
    22. AI Media Dashboard – Interactive charts display AI-detected events and observations
    23. Graphical Weather applet displaying local weather data with satellite and updating radar imaging
    24. Integration of maps, aerial and satellite imagery
    25. Graphical Data Management Tools showing archived and current system status of solar amperage, battery power remaining, wireless radio connectivity and device location
  1. **Security and Management**
     1. Access to account protected by Account Security feature which includes four levels of password protection, IP address block/permission and SSL protection of user login password.
     2. The system shall capture and upload images every 15 minutes, 24 hours per day.
     3. The system shall have M2M – Machine to Machine 24/7 Support with active self-healing technology and automatic software upgrades to maintain the quality, consistency and reliability of all images.
     4. Images will be maintained on the System Vendor’s servers for reference available at all times during the life of the project and for no less than 60 days after completion. All images will be protected on servers owned and operated by the System Vendor and located in a secure area at the System Vendor’s location.

1. **CONTRACTOR REQUIREMENTS** 
   1. **Jobsite Requirements**

The Contractor shall secure a nearby structure for camera mounting or provide a fixed pole (40 foot / 12 meters height recommended) and 3 inch / 8 centimeters minimum diameter as per System Vendor’s instruction. The Contractor shall supply all equipment required for safe and secure access to the camera location for technicians performing installation and maintenance services, including building access, bucket truck and/or lift. The System Vendor will consult on and provide recommendations for optimal camera placement and provide professional installation services as required.

* 1. **Camera Maintenance**

The Contractor shall provide all service and maintenance, including cleaning, of the camera system throughout the life of the project including making appropriate arrangements for camera to remain in operation up to and through finalization of all structural, landscaping and “completed state” condition necessary for beginning-to-end time-lapse record.

1. **DELIVERABLES** 
   1. **Public Website**

The System Vendor shall provide custom public website development. Website shall be separate from the Online Interface, match the look and colors of the project’s website, and be delivered as embed code or standalone web page. Additional features include Facebook and Twitter integration, full screen mode, image comparison, weather, multiple logos, graphical background image and project description.

* 1. **End of Project**

The System Vendor at the end of the project shall provide a comprehensive archive package that includes all images, historical weather data, computer-generated time-lapse movies and a royalty-free web-based viewer software. The software shall include the same interactive interface as the live camera during the project.

* 1. **End of Project Time-Lapse Movie**

The System Vendor shall provide time-lapse movie(s) at the end of the project. Time-lapses shall be professionally edited by a video editor using image stabilization software. The movie will start with a graphic, incorporating project title, date and logo. Periods of bad weather or inactivity shall be removed to produce a compelling and consistent movie. A machine edited movie will not be acceptable.